<https://www.eumetsat.int/website/home/TechnicalBulletins/EUMETCast/DAT_3589215.html>

Since 1 May 2018 EUTELSAT 8W has been used for the new EUMETCast Africa Service. The following table shows the final downlink parameters.

| **PARAMETERS** |  |
| --- | --- |
| Name | EUTELSAT 8W |
| Transponder | C04 |
| Down Link Frequency | 3848.2525 MHz |
| Symbol Rate | 9.892 MS/s |
| Polarisation | Circular Left Hand |
| DVB-S2 MODCOD | 4PSK (QPSK) 3/4 |







